DJI Thermal SDK API v1.4 Infrared camera image processing and temperature measurement library API

Data Fields
dirp_color_bar_t Struct Reference

Color bar parameters structure definition. More...

`#include <dirp_api.h>`

## Data Fields
bool | manual_enable
float | high
float | low

## Detailed Description

Color bar parameters structure definition.

## Field Documentation

## ◆ high

float high

Upper limit. Only effective when color bar is in manual mode.

## ◆ low

float low

Lower limit. Only effective when color bar is in manual mode.

## ◆ manual_enable

bool manual_enable

Color bar mode, manual(true) or automatic(false)

The documentation for this struct was generated from the following file:

- E:/Jenkins/camsw/workspace/farm_prj/farm_gd610_tsdk_commit_pipeline/build_windows/Include/dirp_api.h