DJI Thermal SDK API v1.4 Infrared camera image processing and temperature measurement library API

Data Fields
dirp_measurement_params_t Struct Reference

Customize temperature measurement parameteres structure definition. More...

`#include <dirp_api.h>`

## Data Fields
float | distance
float | humidity
float | emissivity
float | reflection

## Detailed Description

Customize temperature measurement parameteres structure definition.

## Field Documentation

## ◆ distance

float distance

The distance to the target. Value range is [1~25] meters.

## ◆ emissivity

float emissivity

How strongly the target surface is emitting energy as thermal radiation. Value range is [0.10~1.00].

## ◆ humidity

float humidity

The relative humidity of the environment. Value range is [20~100] percent. Defualt value is 70%.

## ◆ reflection

float reflection

Reflected temperature in Celsius. The surface of the target that is measured could reflect the energy radiated by the surrounding objects. Value range is [-40.0~500.0]

The documentation for this struct was generated from the following file:

- E:/Jenkins/camsw/workspace/farm_prj/farm_gd610_tsdk_commit_pipeline/build_windows/Include/dirp_api.h