\hypertarget{structdirp__measurement__params__t}{}\doxysection{dirp\+\_\+measurement\+\_\+params\+\_\+t Struct Reference}
\label{structdirp__measurement__params__t}\index{dirp\_measurement\_params\_t@{dirp\_measurement\_params\_t}}


Customize temperature measurement parameteres structure definition.  




{\ttfamily \#include $<$dirp\+\_\+api.\+h$>$}

\doxysubsection*{Data Fields}
\begin{DoxyCompactItemize}
\item 
float \mbox{\hyperlink{structdirp__measurement__params__t_a06f14a9abd47b91465f895d5259cdc1b}{distance}}
\item 
float \mbox{\hyperlink{structdirp__measurement__params__t_a6a87b2b0cff24d38b367ccd34843a206}{humidity}}
\item 
float \mbox{\hyperlink{structdirp__measurement__params__t_a8c5ceadb9fdb54e5f940d669f90843c0}{emissivity}}
\item 
float \mbox{\hyperlink{structdirp__measurement__params__t_adfc4a7d81f395457c9111e79fdba8e51}{reflection}}
\end{DoxyCompactItemize}


\doxysubsection{Detailed Description}
Customize temperature measurement parameteres structure definition. 

\doxysubsection{Field Documentation}
\mbox{\Hypertarget{structdirp__measurement__params__t_a06f14a9abd47b91465f895d5259cdc1b}\label{structdirp__measurement__params__t_a06f14a9abd47b91465f895d5259cdc1b}} 
\index{dirp\_measurement\_params\_t@{dirp\_measurement\_params\_t}!distance@{distance}}
\index{distance@{distance}!dirp\_measurement\_params\_t@{dirp\_measurement\_params\_t}}
\doxysubsubsection{\texorpdfstring{distance}{distance}}
{\footnotesize\ttfamily float distance}

The distance to the target. Value range is \mbox{[}1$\sim$25\mbox{]} meters. \mbox{\Hypertarget{structdirp__measurement__params__t_a8c5ceadb9fdb54e5f940d669f90843c0}\label{structdirp__measurement__params__t_a8c5ceadb9fdb54e5f940d669f90843c0}} 
\index{dirp\_measurement\_params\_t@{dirp\_measurement\_params\_t}!emissivity@{emissivity}}
\index{emissivity@{emissivity}!dirp\_measurement\_params\_t@{dirp\_measurement\_params\_t}}
\doxysubsubsection{\texorpdfstring{emissivity}{emissivity}}
{\footnotesize\ttfamily float emissivity}

How strongly the target surface is emitting energy as thermal radiation. Value range is \mbox{[}0.\+10$\sim$1.00\mbox{]}. \mbox{\Hypertarget{structdirp__measurement__params__t_a6a87b2b0cff24d38b367ccd34843a206}\label{structdirp__measurement__params__t_a6a87b2b0cff24d38b367ccd34843a206}} 
\index{dirp\_measurement\_params\_t@{dirp\_measurement\_params\_t}!humidity@{humidity}}
\index{humidity@{humidity}!dirp\_measurement\_params\_t@{dirp\_measurement\_params\_t}}
\doxysubsubsection{\texorpdfstring{humidity}{humidity}}
{\footnotesize\ttfamily float humidity}

The relative humidity of the environment. Value range is \mbox{[}20$\sim$100\mbox{]} percent. Defualt value is 70\%. \mbox{\Hypertarget{structdirp__measurement__params__t_adfc4a7d81f395457c9111e79fdba8e51}\label{structdirp__measurement__params__t_adfc4a7d81f395457c9111e79fdba8e51}} 
\index{dirp\_measurement\_params\_t@{dirp\_measurement\_params\_t}!reflection@{reflection}}
\index{reflection@{reflection}!dirp\_measurement\_params\_t@{dirp\_measurement\_params\_t}}
\doxysubsubsection{\texorpdfstring{reflection}{reflection}}
{\footnotesize\ttfamily float reflection}

Reflected temperature in Celsius. The surface of the target that is measured could reflect the energy radiated by the surrounding objects. Value range is \mbox{[}-\/40.\+0$\sim$500.0\mbox{]} 

The documentation for this struct was generated from the following file\+:\begin{DoxyCompactItemize}
\item 
E\+:/\+Jenkins/camsw/workspace/farm\+\_\+prj/farm\+\_\+gd610\+\_\+tsdk\+\_\+commit\+\_\+pipeline/build\+\_\+windows/\+Include/\mbox{\hyperlink{dirp__api_8h}{dirp\+\_\+api.\+h}}\end{DoxyCompactItemize}
